<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="54.59" y2="0" width="0" layer="20"/>
<wire x1="54.59" y1="0" x2="54.59" y2="84.76" width="0" layer="20"/>
<wire x1="54.59" y1="84.76" x2="0" y2="84.76" width="0" layer="20"/>
<wire x1="0" y1="84.76" x2="0" y2="0" width="0" layer="20"/>
<text>panda1</text>
<text>panda2</text>
<hole x="51.6128" y="81.788" drill="2.9972"/>
<hole x="51.6128" y="2.54" drill="2.9972"/>
<hole x="2.794" y="2.54" drill="2.9972"/>
<hole x="2.794" y="62.1538" drill="2.9972"/>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="DCJACK_2MM_PTH">
<description>DJ Jack 2.0mm PTH Right-Angle</description>
</package>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
</packages>
</library>
<library name="comma.ai">
<description>MobileEye connector</description>
<packages>
<package name="OBDII-FEMALE">
<description>OBDII Connector footprint, for your late model automotive needs</description>
</package>
<package name="0603-R">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="AYZ0202">
<description>&lt;b&gt;DPDT Slide Switch SMD&lt;/b&gt;
www.SparkFun.com SKU : Comp-SMDS</description>
</package>
</packages>
</library>
<library name="oldlib">
<description>MobileEye connector</description>
<packages>
<package name="LOGO">
</package>
</packages>
</library>
<library name="comma.ai">
<description>comma.ai's library (duh)</description>
<packages>
<package name="DUMMY">
<description>&lt;h3&gt;Dummy Footprint&lt;/h3&gt;
&lt;p&gt;NOTHING HERE!!! For when you want a symbol with no package as an option against symbols with a package.&lt;/p&gt;

&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;BADGERHACK_LOGO&lt;/li&gt;
&lt;li&gt;FRAME-LETTER&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="12V" library="adafruit" package="DCJACK_2MM_PTH" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="comma.ai" package="OBDII-FEMALE" value="OBDII-FEMALEFEMALE"/>
<element name="J2" library="comma.ai" package="OBDII-FEMALE" value="OBDII-FEMALEFEMALE"/>
<element name="PWR" library="adafruit" package="CHIPLED_0805" value="RED">
<attribute name="NAME"/>
</element>
<element name="R1" library="comma.ai" package="0603-R" value="3.3k">
<attribute name="NAME"/>
</element>
<element name="R2" library="comma.ai" package="0603-R" value="120">
<attribute name="NAME"/>
</element>
<element name="R3" library="comma.ai" package="0603-R" value="120">
<attribute name="NAME"/>
</element>
<element name="R4" library="comma.ai" package="0603-R" value="120">
<attribute name="NAME"/>
</element>
<element name="SW1" library="comma.ai" package="AYZ0202" value="DPDTDPDT"/>
<element name="SW2" library="comma.ai" package="AYZ0202" value="DPDTDPDT"/>
<element name="R5" library="comma.ai" package="0603-R" value="3.3k">
<attribute name="NAME"/>
</element>
<element name="IGN" library="adafruit" package="CHIPLED_0805" value="GREEN">
<attribute name="NAME"/>
</element>
<element name="U$1" library="oldlib" package="LOGO" value=""/>
<element name="FRAME1" library="comma.ai" package="DUMMY" value="FRAME-LETTER-OPENNO_PACKAGE">
<attribute name="DESIGNER" value="Nobody"/>
<attribute name="VERSION" value="v01"/>
</element>
</elements>
<signals>
<signal name="GMLAN">
<contactref element="J1" pad="1"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="CAN2H">
<contactref element="J1" pad="3"/>
<contactref element="J2" pad="3"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="KLIN">
<contactref element="J1" pad="7"/>
<contactref element="J2" pad="7"/>
</signal>
<signal name="CAN2L">
<contactref element="J1" pad="11"/>
<contactref element="J2" pad="11"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="CAN3H">
<contactref element="J1" pad="12"/>
<contactref element="J2" pad="12"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="CAN3L">
<contactref element="J1" pad="13"/>
<contactref element="J2" pad="13"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="CAN1L">
<contactref element="J1" pad="14"/>
<contactref element="J2" pad="14"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="12V">
<contactref element="J1" pad="16"/>
<contactref element="J2" pad="16"/>
<contactref element="R1" pad="2"/>
<contactref element="SW2" pad="2"/>
<contactref element="SW1" pad="2"/>
<contactref element="SW1" pad="5"/>
</signal>
<signal name="LIN">
<contactref element="J2" pad="15"/>
<contactref element="J1" pad="15"/>
</signal>
<signal name="CAN1H">
<contactref element="J2" pad="6"/>
<contactref element="J1" pad="6"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="IGN">
<contactref element="J2" pad="8"/>
<contactref element="J1" pad="8"/>
<contactref element="R5" pad="2"/>
<contactref element="SW2" pad="3"/>
</signal>
<signal name="GND">
<contactref element="12V" pad="GND"/>
<contactref element="PWR" pad="C"/>
<contactref element="IGN" pad="C"/>
<contactref element="12V" pad="GNDBREAK"/>
<contactref element="J1" pad="4"/>
<contactref element="J2" pad="4"/>
<contactref element="J1" pad="5"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="1"/>
<contactref element="PWR" pad="A"/>
</signal>
<signal name="N$3">
<contactref element="R5" pad="1"/>
<contactref element="IGN" pad="A"/>
</signal>
<signal name="N$1">
<contactref element="12V" pad="PWR"/>
<contactref element="SW1" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
