VERSION ""


NS_ :
    NS_DESC_
    CM_
    BA_DEF_
    BA_
    VAL_
    CAT_DEF_
    CAT_
    FILTER
    BA_DEF_DEF_
    EV_DATA_
    ENVVAR_DATA_
    SGTYPE_
    SGTYPE_VAL_
    BA_DEF_SGTYPE_
    BA_SGTYPE_
    SIG_TYPE_REF_
    VAL_TABLE_
    SIG_GROUP_
    SIG_VALTYPE_
    SIGTYPE_VALTYPE_
    BO_TX_BU_
    BA_DEF_REL_
    BA_REL_
    BA_DEF_DEF_REL_
    BU_SG_REL_
    BU_EV_REL_
    BU_BO_REL_
    SG_MUL_VAL_

BS_:

BU_: XXX DSU HCU EPS IPAS CGW BGM

BO_ 36 KINEMATICS: 8 XXX
 SG_ ACCEL_Y : 33|10@0+ (0.03589,-18.375) [0|65535] "m/s^2" XXX
 SG_ YAW_RATE : 1|10@0+ (0.244,-125) [0|65535] "deg/s" XXX
 SG_ ACCEL_X : 17|10@0+ (0.03589,-18.375) [0|65535] "m/s^2" XXX

BO_ 37 STEER_ANGLE_SENSOR: 8 XXX
 SG_ STEER_ANGLE : 3|12@0- (1.5,0) [-500|500] "deg" XXX
 SG_ STEER_FRACTION : 39|4@0- (0.1,0) [-0.7|0.7] "deg" XXX
 SG_ STEER_RATE : 35|12@0- (1,0) [-2000|2000] "deg/s" XXX

BO_ 119 ENG2F41: 6 CGW
 SG_ FDRV : 7|16@0- (2,0) [0|0] "N" Vector__XXX
 SG_ FDRVREAL : 23|13@0- (10,0) [0|0] "N" Vector__XXX
 SG_ XAECT : 39|1@0+ (1,0) [0|0] "" Vector__XXX
 SG_ XFDRVCOL : 38|1@0+ (1,0) [0|0] "" Vector__XXX
 SG_ FDRVSELP : 34|3@0+ (1,0) [0|0] "" Vector__XXX
 SG_ ENG2F41S : 47|8@0+ (1,0) [0|0] "" Vector__XXX

BO_ 120 ENG2F42: 4 CGW
 SG_ FAVLMCHH : 7|16@0- (2,0) [0|0] "N" Vector__XX228X
 SG_ CCRNG : 23|1@0+ (1,0) [0|0] "" Vector__XXX
 SG_ FDRVTYPD : 22|3@0+ (1,0) [0|0] "" Vector__XXX
 SG_ GEARHD : 18|1@0+ (1,0) [0|0] "" Vector__XXX
 SG_ ENG2F42S : 31|8@0+ (1,0) [0|0] "" Vector__XXX

BO_ 166 BRAKE: 8 XXX
 SG_ BRAKE_AMOUNT : 7|8@0+ (1,0) [0|255] "" XXX
 SG_ BRAKE_FORCE : 23|8@0+ (40,0) [0|10200] "N" XXX

BO_ 170 WHEEL_SPEEDS: 8 XXX
 SG_ WHEEL_SPEED_FR_FAULT : 7|1@0+ (1,0) [0|0] "" AFS,FCM,MAV
 SG_ WHEEL_SPEED_FR : 6|15@0+ (0.01,-67.67) [0|0] "km/h" AFS,BSR,DS1,FCM,KSS,MAV,SCS
 SG_ WHEEL_SPEED_FL_FAULT : 23|1@0+ (1,0) [0|0] "" AFS,FCM,MAV
 SG_ WHEEL_SPEED_FL : 22|15@0+ (0.01,-67.67) [0|0] "km/h" AFS,BSR,DS1,FCM,KSS,MAV,SCS
 SG_ WHEEL_SPEED_RR_FAULT : 39|1@0+ (1,0) [0|0] "" AFS,FCM,MAV
 SG_ WHEEL_SPEED_RR : 38|15@0+ (0.01,-67.67) [0|0] "km/h" AFS,BSR,DS1,FCM,KSS,MAV,SCS
 SG_ WHEEL_SPEED_RL_FAULT : 55|1@0+ (1,0) [0|0] "" AFS,FCM,MAV
 SG_ WHEEL_SPEED_RL : 54|15@0+ (0.01,-67.67) [0|0] "km/h" AFS,BSR,DS1,FCM,KSS,MAV,SCS

BO_ 180 SPEED: 8 XXX
 SG_ ENCODER : 39|8@0+ (1,0) [0|255] "" XXX
 SG_ SPEED : 47|16@0+ (0.01,0) [0|250] "km/h" XXX
 SG_ CHECKSUM : 63|8@0+ (1,0) [0|255] "" XXX

BO_ 295 GEAR_PACKET_HYBRID: 8 XXX
 SG_ FDRVREAL : 26|11@0- (25,0) [-25600|25575] "N" XXX
 SG_ UNKNOWN : 55|8@0+ (1,0) [0|255] "" XXX
 SG_ CHECKSUM : 63|8@0+ (1,0) [0|255] "" XXX
 SG_ GEAR : 47|4@0+ (1,0) [0|15] "" XXX

BO_ 353 DSU_SPEED: 7 XXX
 SG_ FORWARD_SPEED : 15|16@0- (0.00390625,-30) [0|255] "km/h" XXX

BO_ 426 VSC1F02: 6 CGW
 SG_ VXFRF : 7|1@0+ (1,0) [0|0] "" AFS,BSR,FCM,MAV
 SG_ VXFRIGS : 6|1@0+ (1,0) [0|0] "" BSR,DS1,FCM,MAV
 SG_ VXFRHDS : 5|1@0+ (1,0) [0|0] "" FCM,KSS,MAV,SCS
 SG_ VXFLF : 2|1@0+ (1,0) [0|0] "" AFS,BSR,FCM,MAV
 SG_ VXFLIGS : 1|1@0+ (1,0) [0|0] "" BSR,DS1,FCM,MAV
 SG_ VXFLHDS : 0|1@0+ (1,0) [0|0] "" FCM,KSS,MAV,SCS
 SG_ VXRRF : 13|1@0+ (1,0) [0|0] "" AFS,BSR,FCM,MAV
 SG_ VXRRIGS : 12|1@0+ (1,0) [0|0] "" BSR,DS1,FCM,MAV
 SG_ VXRRHDS : 11|1@0+ (1,0) [0|0] "" FCM,KSS,MAV,SCS
 SG_ VXRLF : 8|1@0+ (1,0) [0|0] "" AFS,BSR,FCM,MAV
 SG_ VXRLIGS : 23|1@0+ (1,0) [0|0] "" BSR,DS1,FCM,MAV
 SG_ VXRLHDS : 22|1@0+ (1,0) [0|0] "" FCM,KSS,MAV,SCS
 SG_ VSCF02SM : 47|8@0+ (1,0) [0|0] "" AFS,DS1,FCM,MAV

BO_ 452 ENGINE_RPM: 8 CGW
 SG_ RPM : 7|16@0- (0.78125,0) [0|0] "rpm" SCS
 SG_ ENGINE_RUNNING : 27|1@0+ (1,0) [0|1] "" XXX

BO_ 467 PCM_CRUISE_2: 8 XXX
 SG_ BRAKE_PRESSED : 3|1@0+ (1,0) [0|1] "" XXX
 SG_ PCM_FOLLOW_DISTANCE : 12|2@0+ (1,0) [0|3] "" XXX
 SG_ LOW_SPEED_LOCKOUT : 14|2@0+ (1,0) [0|3] "" XXX
 SG_ MAIN_ON : 15|1@0+ (1,0) [0|1] "" XXX
 SG_ SET_SPEED : 23|8@0+ (1,0) [0|255] "km/h" XXX
 SG_ ACC_FAULTED : 47|1@0+ (1,0) [0|1] "" XXX
 SG_ CHECKSUM : 63|8@0+ (1,0) [0|255] "" XXX

BO_ 552 VSC1S29: 4 CGW
 SG_ ICBACT : 7|1@0+ (1,0) [0|0] "" DS1
 SG_ DVS0PCS : 6|15@0- (0.001,0) [0|0] "m/s^2" DS1
 SG_ SM228 : 31|8@0+ (1,0) [0|0] "" DS1

BO_ 560 BRAKE_2: 7 XXX
 SG_ BRAKE_PRESSED : 26|1@0+ (1,0) [0|1] "" XXX

BO_ 581 GAS_PEDAL_HYBRID: 8 XXX
 SG_ GAS_PEDAL : 23|8@0+ (0.005,0) [0|1] "" XXX

BO_ 608 STEER_TORQUE_SENSOR: 8 XXX
 SG_ STEER_TORQUE_EPS : 47|16@0- (1,0) [-32768|32767] "" XXX
 SG_ STEER_TORQUE_DRIVER : 15|16@0- (1,0) [-32768|32767] "" XXX
 SG_ STEER_ANGLE : 31|16@0- (0.0573,0) [-500|500] "" XXX
 SG_ STEER_ANGLE_INITIALIZING : 3|1@0+ (1,0) [0|1] "" XXX
 SG_ STEER_OVERRIDE : 0|1@0+ (1,0) [0|1] "" XXX
 SG_ CHECKSUM : 63|8@0+ (1,0) [0|255] "" XXX

BO_ 614 STEERING_IPAS: 8 IPAS
 SG_ STATE : 7|4@0+ (1,0) [0|15] "" XXX
 SG_ ANGLE : 3|12@0- (1.5,0) [-510|510] "deg" XXX
 SG_ SET_ME_X10 : 23|8@0+ (1,0) [0|255] "" XXX
 SG_ SET_ME_X00 : 31|8@0+ (1,0) [0|255] "" XXX
 SG_ DIRECTION_CMD : 38|2@0+ (1,0) [0|3] "" XXX
 SG_ SET_ME_X40 : 47|8@0+ (1,0) [0|255] "" XXX
 SG_ SET_ME_X00_1 : 55|8@0+ (1,0) [0|255] "" XXX
 SG_ CHECKSUM : 63|8@0+ (1,0) [0|255] "" XXX

BO_ 742 LEAD_INFO: 8 DSU
 SG_ CHECKSUM : 63|8@0+ (1,0) [0|255] "" HCU
 SG_ LEAD_REL_SPEED : 23|12@0- (0.025,0) [-100|100] "m/s" HCU
 SG_ LEAD_LONG_DIST : 7|13@0+ (0.05,0) [0|300] "m" HCU

BO_ 800 VSC1S07: 8 CGW
 SG_ FBKRLY : 6|1@0+ (1,0) [0|0] "" DS1
 SG_ FVSCM : 4|1@0+ (1,0) [0|0] "" DS1
 SG_ FVSCSFT : 3|1@0+ (1,0) [0|0] "" DS1
 SG_ FABS : 2|1@0+ (1,0) [0|0] "" DS1,FCM
 SG_ TSVSC : 1|1@0+ (1,0) [0|0] "" DS1
 SG_ FVSCL : 0|1@0+ (1,0) [0|0] "" DS1
 SG_ RQCSTBKB : 15|1@0+ (1,0) [0|0] "" Vector__XXX
 SG_ PSBSTBY : 14|1@0+ (1,0) [0|0] "" DS1
 SG_ P2BRXMK : 13|1@0+ (1,0) [0|0] "" DS1
 SG_ MCC : 11|1@0+ (1,0) [0|0] "" DS1
 SG_ RQBKB : 10|1@0+ (1,0) [0|0] "" Vector__XXX
 SG_ BRSTOP : 9|1@0+ (1,0) [0|0] "" DS1,FCM
 SG_ BRKON : 8|1@0+ (1,0) [0|0] "" DS1,FCM
 SG_ ASLP : 23|8@0- (1,0) [0|0] "deg" DS1
 SG_ BRTYPACC : 31|2@0+ (1,0) [0|0] "" DS1
 SG_ BRKABT3 : 26|1@0+ (1,0) [0|0] "" Vector__XXX
 SG_ BRKABT2 : 25|1@0+ (1,0) [0|0] "" Vector__XXX
 SG_ BRKABT1 : 24|1@0+ (1,0) [0|0] "" Vector__XXX
 SG_ GVC : 39|8@0- (0.04,0) [0|0] "m/s^2" DS1
 SG_ XGVCINV : 43|1@0+ (1,0) [0|0] "" DS1
 SG_ S07CNT : 52|1@0+ (1,0) [0|0] "" Vector__XXX
 SG_ PCSBRSTA : 50|2@0+ (1,0) [0|0] "" DS1
 SG_ VSC07SUM : 63|8@0+ (1,0) [0|0] "" DS1,FCM

BO_ 835 ACC_CONTROL: 8 DSU
 SG_ ACCEL_CMD : 7|16@0- (0.001,0) [-20|20] "m/s^2" HCU
 SG_ ALLOW_LONG_PRESS : 17|2@0+ (1,0) [0|2] "" XXX
 SG_ ACC_MALFUNCTION : 18|1@0+ (1,0) [0|0] "" XXX
 SG_ RADAR_DIRTY : 19|1@0+ (1,0) [0|1] "" XXX
 SG_ DISTANCE : 20|1@0+ (1,0) [0|1] "" XXX
 SG_ MINI_CAR : 21|1@0+ (1,0) [0|1] "" XXX
 SG_ ACC_TYPE : 23|2@0+ (1,0) [0|3] "" HCU
 SG_ CANCEL_REQ : 24|1@0+ (1,0) [0|1] "" HCU
 SG_ ACC_CUT_IN : 25|1@0+ (1,0) [0|1] "" XXX
 SG_ LEAD_VEHICLE_STOPPED : 29|1@0+ (1,0) [0|0] "" DSU
 SG_ PERMIT_BRAKING : 30|1@0+ (1,0) [0|1] "" HCU
 SG_ RELEASE_STANDSTILL : 31|1@0+ (1,0) [0|1] "" HCU
 SG_ ITS_CONNECT_LEAD : 39|8@0+ (1,0) [0|1] "" Vector__XXX
 SG_ ACCEL_CMD_ALT : 47|8@0- (0.05,0) [0|0] "m/s^2" XXX
 SG_ CHECKSUM : 63|8@0+ (1,0) [0|255] "" XXX

BO_ 865 CLUTCH: 8 XXX
 SG_ ACC_FAULTED : 32|1@0+ (1,0) [0|1] "" XXX
 SG_ GAS_PEDAL_ALT : 23|8@0+ (0.005,0) [0|1] "" XXX
 SG_ CLUTCH_RELEASED : 38|1@0+ (1,0) [0|1] "" XXX
 SG_ ACCEL_NET : 48|16@1+ (0.0002,-6.5536) [-6.5536|6.5534] "" XXX

BO_ 869 DSU_CRUISE : 7 DSU
 SG_ RES_BTN : 3|1@0+ (1,0) [0|0] "" XXX
 SG_ SET_BTN : 2|1@0+ (1,0) [0|0] "" XXX
 SG_ CANCEL_BTN : 1|1@0+ (1,0) [0|0] "" XXX
 SG_ MAIN_ON : 0|1@0+ (1,0) [0|0] "" XXX
 SG_ SET_SPEED : 15|8@0+ (1,0) [0|0] "km/h" XXX
 SG_ CRUISE_REQUEST : 31|8@0+ (100,-12800) [0|0] "N" XXX
 SG_ LEAD_DISTANCE : 39|8@0+ (1,0) [0|0] "m" XXX

BO_ 898 AIR_CONDITIONER: 8 XXX
 SG_ CLIMATE_SET_POINT : 5|6@0+ (1,0) [5|33] "" XXX
 SG_ AIR_CONDITIONER_STATE : 48|7@1+ (1,0) [0|127] "" XXX

BO_ 921 PCM_CRUISE_SM: 8 XXX
 SG_ MAIN_ON : 4|1@0+ (1,0) [0|1] "" XXX
 SG_ CRUISE_CONTROL_STATE : 11|4@0+ (1,0) [0|15] "" XXX
 SG_ DISTANCE_LINES : 14|2@0+ (1,0) [0|3] "" XXX
 SG_ TEMP_ACC_FAULTED : 15|1@0+ (1,0) [0|1] "" XXX
 SG_ UI_SET_SPEED : 31|8@0+ (1,0) [0|255] "" XXX

BO_ 944 AIR_CONDITIONER_2: 8 XXX
 SG_ WINDSCREEN_DEFOG : 43|1@0+ (1,0) [0|1] "" XXX

BO_ 951 ESP_CONTROL: 8 ESP
 SG_ TC_DISABLED : 13|1@0+ (1,0) [0|1] "" XXX
 SG_ VSC_DISABLED : 12|2@0+ (1,0) [0|1] "" XXX
 SG_ BRAKE_LIGHTS_ACC : 18|1@0+ (1,0) [0|1] "" XXX
 SG_ BRAKE_HOLD_ENABLED : 33|1@1+ (1,0) [0|1] "" XXX
 SG_ BRAKE_HOLD_ACTIVE : 36|1@0+ (1,0) [0|1] "" XXX

BO_ 956 GEAR_PACKET: 8 XXX
 SG_ SPORT_ON : 2|1@0+ (1,0) [0|1] "" XXX
 SG_ GEAR : 13|6@0+ (1,0) [0|63] "" XXX
 SG_ SPORT_GEAR_ON : 33|1@0+ (1,0) [0|1] "" XXX
 SG_ SPORT_GEAR : 38|3@0+ (1,0) [0|7] "" XXX
 SG_ ECON_ON : 40|1@0+ (1,0) [0|1] "" XXX
 SG_ B_GEAR_ENGAGED : 41|1@0+ (1,0) [0|1] "" XXX
 SG_ DRIVE_ENGAGED : 47|1@0+ (1,0) [0|1] "" XXX

BO_ 1005 REVERSE_CAMERA_STATE: 2 BGM
 SG_ REVERSE_CAMERA_GUIDELINES : 9|2@0+ (1,0) [1|3] "" XXX

BO_ 1009 PCM_CRUISE_ALT: 8 XXX
 SG_ PCM_FOLLOW_DISTANCE : 4|2@1+ (1,0) [0|3] "" XXX
 SG_ MAIN_ON : 13|1@0+ (1,0) [0|3] "" XXX
 SG_ CRUISE_STATE : 10|1@0+ (1,0) [0|1] "" XXX
 SG_ UI_SET_SPEED : 23|8@0+ (1,0) [0|255] "mph" XXX

BO_ 1020 SOLAR_SENSOR: 8 XXX
 SG_ LUX_SENSOR : 55|13@0+ (1,0) [0|0] "" XXX

BO_ 1041 PCS_HUD: 8 DSU
 SG_ PCS_INDICATOR : 7|2@0+ (1,0) [0|3] "" XXX
 SG_ FCW : 4|1@0+ (1,0) [0|1] "" XXX
 SG_ SET_ME_X20 : 15|8@0+ (1,0) [0|1] "" XXX
 SG_ PCS_DUST : 34|1@0+ (1,0) [0|0] "" XXX
 SG_ PCS_TEMP : 35|1@0+ (1,0) [0|0] "" XXX
 SG_ PCS_DUST2 : 41|1@0+ (1,0) [0|0] "" XXX
 SG_ PCS_TEMP2 : 42|1@0+ (1,0) [0|0] "" XXX
 SG_ SET_ME_X10 : 39|8@0+ (1,0) [0|1] "" XXX
 SG_ PCS_OFF : 40|1@0+ (1,0) [0|0] "" XXX
 SG_ FRD_ADJ : 53|3@0+ (1,0) [0|0] "" XXX
 SG_ PCS_SENSITIVITY : 55|8@0+ (1,0) [0|1] "" XXX

BO_ 1042 LKAS_HUD: 8 DSU
 SG_ BARRIERS : 1|2@0+ (1,0) [0|3] "" XXX
 SG_ RIGHT_LINE : 3|2@0+ (1,0) [0|3] "" XXX
 SG_ LEFT_LINE : 5|2@0+ (1,0) [0|3] "" XXX
 SG_ LKAS_STATUS : 7|2@0+ (1,0) [0|3] "" XXX
 SG_ LDA_ALERT : 9|2@0+ (1,0) [0|3] "" XXX
 SG_ LDW_EXIST : 10|1@0+ (1,0) [0|1] "" XXX
 SG_ TWO_BEEPS : 12|1@0+ (1,0) [0|1] "" XXX
 SG_ ADJUSTING_CAMERA : 13|1@0+ (1,0) [0|1] "" XXX
 SG_ LDA_UNAVAILABLE_QUIET : 14|1@0+ (1,0) [0|1] "" XXX
 SG_ LDA_MALFUNCTION : 15|1@0+ (1,0) [0|1] "" XXX
 SG_ LDA_UNAVAILABLE : 16|1@0+ (1,0) [0|1] "" XXX
 SG_ LDA_SENSITIVITY : 18|2@0+ (1,0) [0|3] "" XXX
 SG_ LDA_SA_TOGGLE : 20|2@0+ (1,0) [0|3] "" XXX
 SG_ LDA_MESSAGES : 23|3@0+ (1,0) [0|1] "" XXX
 SG_ LDA_ON_MESSAGE : 31|2@0+ (1,0) [0|3] "" XXX
 SG_ REPEATED_BEEPS : 32|1@0+ (1,0) [0|1] "" XXX
 SG_ LANE_SWAY_TOGGLE : 43|1@0+ (1,0) [0|1] "" XXX
 SG_ LANE_SWAY_SENSITIVITY : 45|2@0+ (1,0) [0|3] "" XXX
 SG_ TAKE_CONTROL : 46|1@0+ (1,0) [0|1] "" XXX
 SG_ LDA_FRONT_CAMERA_BLOCKED : 47|1@0+ (1,0) [0|1] "" XXX
 SG_ LANE_SWAY_BUZZER : 50|2@0+ (1,0) [0|0] "" XXX
 SG_ LANE_SWAY_FLD : 53|3@0+ (1,0) [0|7] "" XXX
 SG_ LANE_SWAY_WARNING : 55|2@0+ (1,0) [0|3] "" XXX
 SG_ SET_ME_X01 : 42|1@0+ (1,0) [0|1] "" XXX
 SG_ SET_ME_X02 : 63|8@0+ (1,0) [0|1] "" XXX

BO_ 1043 TIME : 8 CGW
 SG_ YEAR : 7|8@0+ (1,0) [0|0] "year" XXX
 SG_ MONTH : 15|8@0+ (1,0) [0|0] "month" XXX
 SG_ DAY : 23|8@0+ (1,0) [0|0] "day" XXX
 SG_ HOUR : 31|8@0+ (1,0) [0|0] "hour" XXX
 SG_ MINUTE : 39|8@0+ (1,0) [0|0] "minute" XXX
 SG_ GMT_DIFF : 55|1@0+ (1,0) [0|0] "" XXX
 SG_ GMTDIFF_HOURS : 54|4@0+ (1,0) [0|0] "hours" XXX
 SG_ GMTDIFF_MINUTES : 50|6@0+ (1,0) [0|0] "minutes" XXX
 SG_ SUMMER : 60|1@0+ (1,0) [0|0] "" XXX

BO_ 1044 AUTO_HIGH_BEAM: 8 FCM
 SG_ AHB_DUTY : 47|8@0+ (0.5,0) [0|0] "%" Vector__XXX
 SG_ F_AHB : 55|4@0+ (1,0) [0|0] "" Vector__XXX
 SG_ C_AHB : 51|4@0+ (1,0) [0|0] "" Vector__XXX

BO_ 1056 VSC1S08: 8 CGW
 SG_ YR1Z : 7|16@0- (1,0) [0|0] "rad/s" DS1,FCM,MAV
 SG_ YR2Z : 23|16@0- (1,0) [0|0] "rad/s" DS1,FCM,MAV
 SG_ GL1Z : 39|8@0- (0.0359,0) [0|0] "m/s^2" DS1,FCM,KSS,MAV,SCS
 SG_ GL2Z : 47|8@0- (0.0359,0) [0|0] "m/s^2" DS1,FCM,KSS,MAV,SCS
 SG_ YRGSDIR : 55|1@0+ (1,0) [0|0] "" DS1,FCM,KSS,SCS
 SG_ GLZS : 51|1@0+ (1,0) [0|0] "" DS1,FCM,KSS,MAV,SCS
 SG_ YRZF : 50|1@0+ (1,0) [0|0] "" DS1,FCM,MAV
 SG_ YRZS : 49|1@0+ (1,0) [0|0] "" DS1,FCM,MAV
 SG_ YRZKS : 48|1@0+ (1,0) [0|0] "" DS1,FCM,MAV
 SG_ VSC08SUM : 63|8@0+ (1,0) [0|0] "" DS1,FCM,MAV

BO_ 1083 AUTOPARK_STATUS: 8 IPAS
 SG_ STATE : 7|4@0+ (1,0) [0|15] "" XXX

BO_ 1161 RSA1: 8 FCM
 SG_ TSGN1 : 7|8@0+ (1,0) [0|0] "" XXX
 SG_ TSGNGRY1 : 12|3@0+ (1,0) [0|0] "" XXX
 SG_ TSGNHLT1 : 9|2@0+ (1,0) [0|0] "" XXX
 SG_ SPDVAL1 : 23|8@0+ (1,0) [0|0] "km/h" XXX
 SG_ SPLSGN1 : 31|4@0+ (1,0) [0|0] "" XXX
 SG_ SPLSGN2 : 27|4@0+ (1,0) [0|0] "" XXX
 SG_ TSGN2 : 39|8@0+ (1,0) [0|0] "" XXX
 SG_ TSGNGRY2 : 44|3@0+ (1,0) [0|0] "" XXX
 SG_ TSGNHLT2 : 41|2@0+ (1,0) [0|0] "" XXX
 SG_ SPDVAL2 : 55|8@0+ (1,0) [0|0] "" XXX
 SG_ BZRRQ_P : 63|2@0+ (1,0) [0|0] "" XXX
 SG_ BZRRQ_A : 61|2@0+ (1,0) [0|0] "" XXX
 SG_ SYNCID1 : 59|4@0+ (1,0) [0|0] "" XXX

BO_ 1162 RSA2: 8 FCM
 SG_ TSGN3 : 7|8@0+ (1,0) [0|0] "" XXX
 SG_ TSGNGRY3 : 12|3@0+ (1,0) [0|0] "" XXX
 SG_ TSGNHLT3 : 9|2@0+ (1,0) [0|0] "" XXX
 SG_ SPLSGN3 : 31|4@0+ (1,0) [0|0] "" XXX
 SG_ SPLSGN4 : 27|4@0+ (1,0) [0|0] "" XXX
 SG_ TSGN4 : 39|8@0+ (1,0) [0|0] "" XXX
 SG_ TSGNGRY4 : 44|3@0+ (1,0) [0|0] "" XXX
 SG_ TSGNHLT4 : 41|2@0+ (1,0) [0|0] "" XXX
 SG_ DPSGNREQ : 54|1@0+ (1,0) [0|0] "" XXX
 SG_ SGNNUMP : 53|3@0+ (1,0) [0|0] "" XXX
 SG_ SGNNUMA : 50|3@0+ (1,0) [0|0] "" XXX
 SG_ SPDUNT : 63|2@0+ (1,0) [0|0] "" XXX
 SG_ TSRWMSG : 61|2@0+ (1,0) [0|0] "" XXX
 SG_ SYNCID2 : 59|4@0+ (1,0) [0|0] "" XXX

BO_ 1163 RSA3: 8 FCM
 SG_ TSREQPD : 7|1@0+ (1,0) [0|0] "" XXX
 SG_ TSRMSW : 6|1@0+ (1,0) [0|0] "" XXX
 SG_ OTSGNNTM : 5|2@0+ (1,0) [0|0] "" XXX
 SG_ NTLVLSPD : 3|2@0+ (1,0) [0|0] "" XXX
 SG_ OVSPNTM : 1|2@0+ (1,0) [0|0] "" XXX
 SG_ OVSPVALL : 11|4@0+ (1,-5) [0|0] "" XXX
 SG_ OVSPVALM : 19|4@0+ (1,-5) [0|0] "" XXX
 SG_ OVSPVALH : 27|4@0+ (1,-5) [0|0] "" XXX
 SG_ TSRSPU : 33|2@0+ (1,0) [0|0] "" XXX

BO_ 1408 VIN_PART_1: 8 CGW
 SG_ VIN_1 : 7|8@0+ (1,0) [0|0] "" XXX
 SG_ VIN_2 : 15|8@0+ (1,0) [0|0] "" XXX
 SG_ VIN_3 : 23|8@0+ (1,0) [0|0] "" XXX
 SG_ VIN_4 : 31|8@0+ (1,0) [0|0] "" XXX
 SG_ VIN_5 : 39|8@0+ (1,0) [0|0] "" XXX
 SG_ VIN_6 : 47|8@0+ (1,0) [0|0] "" XXX
 SG_ VIN_7 : 55|8@0+ (1,0) [0|0] "" XXX
 SG_ VIN_8 : 63|8@0+ (1,0) [0|0] "" XXX

BO_ 1409 VIN_PART_2: 8 CGW
 SG_ VIN_9 : 7|8@0+ (1,0) [0|0] "" XXX
 SG_ VIN_10 : 15|8@0+ (1,0) [0|0] "" XXX
 SG_ VIN_11 : 23|8@0+ (1,0) [0|0] "" XXX
 SG_ VIN_12 : 31|8@0+ (1,0) [0|0] "" XXX
 SG_ VIN_13 : 39|8@0+ (1,0) [0|0] "" XXX
 SG_ VIN_14 : 47|8@0+ (1,0) [0|0] "" XXX
 SG_ VIN_15 : 55|8@0+ (1,0) [0|0] "" XXX
 SG_ VIN_16 : 63|8@0+ (1,0) [0|0] "" XXX

BO_ 1410 VIN_PART_3: 8 CGW
 SG_ VIN_17 : 7|8@0+ (1,0) [0|0] "" XXX

BO_ 1552 BODY_CONTROL_STATE_2: 8 XXX
 SG_ UI_SPEED : 23|8@0+ (1,0) [0|255] "" XXX
 SG_ METER_SLIDER_BRIGHTNESS_PCT : 30|7@0+ (1,0) [12|100] "%" XXX
 SG_ METER_SLIDER_LOW_BRIGHTNESS : 37|1@0+ (1,0) [0|1] "" XXX
 SG_ METER_SLIDER_DIMMED : 38|1@0+ (1,0) [0|1] "" XXX
 SG_ UNITS : 63|3@0+ (1,0) [1|4] "" XXX

BO_ 1553 UI_SETTING: 8 XXX
 SG_ UNITS : 26|2@0+ (1,0) [0|3] "" XXX
 SG_ ODOMETER : 39|32@0+ (1,0) [0|1048575] "" XXX

BO_ 1556 BLINKERS_STATE: 8 XXX
 SG_ BLINKER_BUTTON_PRESSED : 15|1@0+ (1,0) [0|1] "" XXX
 SG_ HAZARD_LIGHT : 27|1@0+ (1,0) [0|1] "" XXX
 SG_ TURN_SIGNALS : 29|2@0+ (1,0) [0|3] "" XXX

BO_ 1568 BODY_CONTROL_STATE: 8 XXX
 SG_ METER_DIMMED : 38|1@0+ (1,0) [0|1] "" XXX
 SG_ PARKING_BRAKE : 60|1@0+ (1,0) [0|1] "" XXX
 SG_ SEATBELT_DRIVER_UNLATCHED : 62|1@0+ (1,0) [0|1] "" XXX
 SG_ DOOR_OPEN_FL : 45|1@0+ (1,0) [0|1] "" XXX
 SG_ DOOR_OPEN_RL : 42|1@0+ (1,0) [0|1] "" XXX
 SG_ DOOR_OPEN_RR : 43|1@0+ (1,0) [0|1] "" XXX
 SG_ DOOR_OPEN_FR : 44|1@0+ (1,0) [0|1] "" XXX

BO_ 1570 LIGHT_STALK: 8 SCM
 SG_ LIGHT_STALK_MOVED : 15|1@0+ (1,0) [0|1] "" XXX
 SG_ TAIL_LIGHT : 19|1@0+ (1,0) [0|1] "" XXX
 SG_ HEADLIGHT_MODE : 21|3@1+ (1,0) [0|7] "" XXX
 SG_ FRONT_FOG : 27|1@0+ (1,0) [0|1] "" XXX
 SG_ PARKING_LIGHT : 28|1@0+ (1,0) [0|1] "" XXX
 SG_ LOW_BEAM : 29|1@0+ (1,0) [0|1] "" XXX
 SG_ HIGH_BEAM : 30|1@0+ (1,0) [0|1] "" XXX
 SG_ DAYTIME_RUNNING_LIGHT : 31|1@0+ (1,0) [0|1] "" XXX
 SG_ AUTO_HIGH_BEAM : 37|1@0+ (1,0) [0|1] "" XXX

BO_ 1571 CERTIFICATION_ECU: 8 CGW
 SG_ DOOR_LOCK_FEEDBACK_LIGHT : 15|1@0+ (1,0) [0|0] "" XXX
 SG_ KEYFOB_LOCKING_FEEDBACK_LIGHT : 61|1@0+ (1,0) [0|0] "" XXX
 SG_ KEYFOB_UNLOCKING_FEEDBACK_LIGHT : 62|1@0+ (1,0) [0|0] "" XXX

BO_ 1592 DOOR_LOCKS: 8 XXX
 SG_ LOCK_STATUS_CHANGED : 15|1@0+ (1,0) [0|1] "" XXX
 SG_ LOCK_STATUS : 20|1@0+ (1,0) [0|1] "" XXX
 SG_ LOCKED_VIA_KEYFOB : 23|1@0+ (1,0) [0|1] "" XXX

BO_ 1779 ADAS_TOGGLE_STATE: 8 XXX
 SG_ OK_BUTTON_PRESSED : 15|1@0+ (1,0) [0|1] "" BCM
 SG_ SWS_TOGGLE_CMD : 24|1@0+ (1,0) [0|1] "" XXX
 SG_ SWS_SENSITIVITY_CMD : 26|2@0+ (1,0) [0|3] "" XXX
 SG_ LKAS_ON_CMD : 28|1@0+ (1,0) [0|1] "" XXX
 SG_ LKAS_OFF_CMD : 29|1@0+ (1,0) [0|1] "" XXX
 SG_ LDA_SENSITIVITY_HI_CMD : 30|1@0+ (1,0) [0|1] "" XXX
 SG_ LDA_SENSITIVITY_STD_CMD : 31|1@0+ (1,0) [0|1] "" XXX
 SG_ IPAS_TOGGLE : 34|1@0+ (1,0) [0|1] "" XXX
 SG_ BSM_TOGGLE_CMD : 37|1@0+ (1,0) [0|1] "" XXX
 SG_ IPAS_SONAR_TOGGLE : 38|1@0+ (1,0) [0|1] "" XXX
 SG_ PCS_TOGGLE_CMD : 40|1@0+ (1,0) [0|1] "" XXX
 SG_ PCS_SENSITIVITY_CMD : 41|1@0+ (1,0) [0|1] "" XXX

CM_ SG_ 36 YAW_RATE "verify";
CM_ SG_ 36 ACCEL_X "x-axis accel";
CM_ SG_ 37 STEER_FRACTION "1/15th of the signal STEER_ANGLE, which is 1.5 deg; note that 0x8 is never set";
CM_ SG_ 37 STEER_RATE "factor is tbd";
CM_ SG_ 119 FDRVREAL "ICE only: force applied by wheels from the engine. includes creeping force, regen, and engine braking";
CM_ SG_ 166 BRAKE_FORCE "hybrid only: force applied by friction brakes from user or ACC command";
CM_ SG_ 295 FDRVREAL "hybrid only: force applied by wheels from the engine and/or electric motors. includes creeping force, regen, and engine braking";
CM_ SG_ 467 ACC_FAULTED "1 when ACC is faulted and the PCM disallows engagement";
CM_ SG_ 467 SET_SPEED "43 km/h are shown as 28 mph, so conversion isn't perfect";
CM_ SG_ 467 LOW_SPEED_LOCKOUT "in low speed lockout, system would always disengage below 28mph";
CM_ SG_ 560 BRAKE_PRESSED "another brake pressed?";
CM_ SG_ 581 GAS_PEDAL "it seems slightly filtered";
CM_ SG_ 608 STEER_TORQUE_DRIVER "driver torque";
CM_ SG_ 608 STEER_OVERRIDE "set when driver torque exceeds a certain value";
CM_ SG_ 614 ANGLE "set to measured angle when ipas control isn't active";
CM_ SG_ 835 ACC_TYPE "if 2, car is likely to have a permanent low speed lockout. 1 is ok";
CM_ SG_ 835 RADAR_DIRTY "Display Clean Radar Sensor message on HUD";
CM_ SG_ 835 ACC_MALFUNCTION "display ACC fault on dash if set to 1";
CM_ SG_ 835 ACC_CUT_IN "Display blinking yellow lead if set to 1";
CM_ SG_ 835 DISTANCE "Cycle through ACC following distance from long, mid, short when set to 1";
CM_ SG_ 835 ITS_CONNECT_LEAD "Displayed when lead car is capable of ITS Connect";
CM_ SG_ 835 LEAD_VEHICLE_STOPPED "Set to 1 when lead is stopped, likely only used in older TSS-P vehicles";
CM_ SG_ 835 ALLOW_LONG_PRESS "Enable Toyota's factory set speed increment behaviour, available on both metrics cars and imperial unit cars";
CM_ SG_ 835 PERMIT_BRAKING "Original ACC has this going high when a car in front is detected. In openpilot and before the PERMIT_BRAKING name, this was 'SET_ME_1' and is hardcoded to be high. Unsure if only informational or has an effect though existing usage in openpilot is to always set it to 1. Originally 'PMTBRKG' in the leaked toyota_2017_ref_pt.dbc file and name expansion speculated to be PerMiT BRaKinG.";
CM_ SG_ 835 ACCEL_CMD_ALT "Copy of main ACCEL_CMD, but across 8 bits instead of 16 bits like ACCEL_CMD. Unsure if only informational or has an effect. Likely informational as existing openpilot sets this to 0 and no loss of functionality observed. Originally 'AT_RAW' in leaked toyota_2017_ref_pt.dbc file.";
CM_ SG_ 865 GAS_PEDAL_ALT "copy of main GAS_PEDAL. Both use 8 bits. Might indicate that this message is for pedals.";
CM_ SG_ 865 CLUTCH_RELEASED "boolean of clutch for 6MT.";
CM_ SG_ 865 ACCEL_NET "net positive acceleration (gas) applied by the system if on flat ground, may not include creeping force";
CM_ SG_ 865 ACC_FAULTED "1 when ACC is faulted and the PCM disallows engagement. Also describes a lockout when the ACC_CONTROL->ACC_MALFUNCTION bit is set.";
CM_ SG_ 898 AIR_CONDITIONER_STATE "very difficult to parse with some air register motors operating without user-inputs";
CM_ SG_ 921 UI_SET_SPEED "set speed shown in the vehicle's UI with the vehicle's unit";
CM_ SG_ 921 TEMP_ACC_FAULTED "1 when the UI is displaying or playing fault-related alerts or sounds. Also 1 when pressing main on.";
CM_ SG_ 951 BRAKE_LIGHTS_ACC "brake lights when ACC commands decel";
CM_ SG_ 956 GEAR "on 6MT, only R shows.";
CM_ SG_ 1009 UI_SET_SPEED "units seem to be whatever the car is set to";
CM_ SG_ 1041 PCS_INDICATOR "Pre-Collision System Indicator";
CM_ SG_ 1041 PCS_SENSITIVITY "Pre-Collision System Sensitivity";
CM_ SG_ 1041 PCS_DUST "alert: Front Camera Low Visibility Unavailable See Owner's Manual";
CM_ SG_ 1041 PCS_DUST2 "alert: Pre-Collision System Radar Sensor Blocked Unavailable Clean Radar Sensor";
CM_ SG_ 1041 PCS_TEMP "alert: Front Camera Out of Temperature Range Unavailable Wait until Normal Temperature";
CM_ SG_ 1041 PCS_TEMP2 "alert: Pre-Collision System Out of Temperature Range Unavailable See Owner's Manual";
CM_ SG_ 1041 FRD_ADJ "alert: ERROR ADJUSTING FRONT RADAR BEAM";
CM_ SG_ 1042 LDA_SA_TOGGLE "LDA Steering Assist Toggle";
CM_ SG_ 1042 LDW_EXIST "Unclear what this is, it's usually set to 0";
CM_ SG_ 1042 LDA_SENSITIVITY "LDA Sensitivity";
CM_ SG_ 1042 LDA_ON_MESSAGE "Display LDA Turned ON message";
CM_ SG_ 1042 REPEATED_BEEPS "LDA audible warning";
CM_ SG_ 1042 LDA_UNAVAILABLE_QUIET "LDA toggles and sensitivity settings are greyed out if set to 1";
CM_ SG_ 1042 LDA_MESSAGES "Various LDA Messages";
CM_ SG_ 1042 LDA_FRONT_CAMERA_BLOCKED "originally LDAFCVB, LDA related settings are greyed out if set to 1";
CM_ SG_ 1042 TAKE_CONTROL "Please Control Steering Wheel warning";
CM_ SG_ 1042 LANE_SWAY_TOGGLE "Lane Sway Warning System SWS Switch";
CM_ SG_ 1042 LANE_SWAY_WARNING "Lane Sway Warning System Triggered";
CM_ SG_ 1042 LANE_SWAY_FLD "Unknown signal for Lane Sway Warning System, set to 7 on stock system when SWS is enabled, 0 when SWS is disabled";
CM_ SG_ 1042 LANE_SWAY_BUZZER "Similar to TWO_BEEPS";
CM_ SG_ 1042 SET_ME_X01 "empty bit on leaked dbc, always set to 1 during normal operations";
CM_ SG_ 1042 SET_ME_X02 "empty bit on leaked dbc, always set to 2 during normal operations";
CM_ SG_ 1083 STATE "when the dashboard button is pressed, the value changes from zero to non-zero";
CM_ SG_ 1161 SPDVAL1 "Numbers 0-199 is displayed, 200-254 displays circle without number and 255 is for no limit.";
CM_ SG_ 1161 SYNCID1 "counter from 1 to f at 1 Hz";
CM_ SG_ 1161 SPDVAL2 "conditional speed value 70";
CM_ SG_ 1162 SGNNUMP "1 if SPDVAL1 is set, otherwise 0";
CM_ SG_ 1162 SYNCID2 "counter from 1 to f at 1 Hz";
CM_ SG_ 1163 TSREQPD "always 1";
CM_ SG_ 1163 TSRMSW "always 1";
CM_ SG_ 1163 OTSGNNTM "always 3";
CM_ SG_ 1163 NTLVLSPD "always 3";
CM_ SG_ 1163 OVSPNTM "always 3";
CM_ SG_ 1163 OVSPVALL "-5 at start then 2 after 2 seconds";
CM_ SG_ 1163 OVSPVALM "-5 at start then 5 after 2 seconds";
CM_ SG_ 1163 OVSPVALH "-5 at start then 10 after 2 seconds";
CM_ SG_ 1163 TSRSPU "always 1";
CM_ SG_ 1552 UI_SPEED "Does not appear to match dash";
CM_ SG_ 1552 METER_SLIDER_BRIGHTNESS_PCT "Combination display brightness setting, scales from 12 per cent to 100 per cent, reflects combination meter settings only, not linked with headlight state";
CM_ SG_ 1552 METER_SLIDER_LOW_BRIGHTNESS "Combination display low brightness mode, also controls footwell lighting";
CM_ SG_ 1552 METER_SLIDER_DIMMED "Combination display slider not at max, reflects combination meter settings only, not linked with headlight state";
CM_ SG_ 1553 ODOMETER "Unit is dependent upon units signal";
CM_ SG_ 1592 LOCK_STATUS_CHANGED "1 on rising edge of lock/unlocking";
CM_ SG_ 1592 LOCK_STATUS "The next 3 bits always seem to follow this signal.";
CM_ SG_ 1592 LOCKED_VIA_KEYFOB "1 for as long as car is locked with key fob or door handle touch";

VAL_ 295 GEAR 0 "P" 1 "R" 2 "N" 3 "D" 4 "B";
VAL_ 467 LOW_SPEED_LOCKOUT 2 "low speed locked" 1 "ok";
VAL_ 467 PCM_FOLLOW_DISTANCE 1 "far" 2 "medium" 3 "close";
VAL_ 614 STATE 3 "enabled" 1 "disabled";
VAL_ 614 DIRECTION_CMD 3 "right" 2 "center" 1 "left";
VAL_ 835 ACC_TYPE 2 "permanent low speed lockout" 1 "ok";
VAL_ 835 ACC_MALFUNCTION 1 "faulted" 0 "ok";
VAL_ 835 ACC_CUT_IN 1 "CUT-IN Detected" 0 "clear";
VAL_ 835 ALLOW_LONG_PRESS 2 "set speed increase by 5 speed units regardless" 1 "set speed increase by 1 speed unit on short press, 5 speed units on long press";
VAL_ 865 CLUTCH_RELEASED 0 "clutch pressed any amount" 1 "clutch released";
VAL_ 898 CLIMATE_SET_POINT 0 "CLIMATE LO MODE" 55 "CLIMATE HI MODE" 57 "CLIMATE OFF";
VAL_ 898 AIR_CONDITIONER_STATE 20 "CLIMATE OFF";
VAL_ 921 CRUISE_CONTROL_STATE 2 "disabled" 11 "hold" 10 "hold_waiting_user_cmd" 6 "enabled" 5 "faulted";
VAL_ 921 DISTANCE_LINES 0 "not displayed" 1 "close" 2 "medium" 3 "far";
VAL_ 956 SPORT_ON 0 "off" 1 "on";
VAL_ 956 GEAR 0 "D" 1 "S" 8 "N" 16 "R" 32 "P";
VAL_ 956 SPORT_GEAR_ON 0 "off" 1 "on";
VAL_ 956 SPORT_GEAR 1 "S1" 2 "S2" 3 "S3" 4 "S4" 5 "S5" 6 "S6";
VAL_ 956 ECON_ON 0 "off" 1 "on";
VAL_ 956 B_GEAR_ENGAGED 0 "off" 1 "on";
VAL_ 956 DRIVE_ENGAGED 0 "off" 1 "on";
VAL_ 1005 REVERSE_CAMERA_GUIDELINES 3 "No guidelines" 2 "Static guidelines" 1 "Active guidelines";
VAL_ 1009 PCM_FOLLOW_DISTANCE 1 "far" 2 "medium" 3 "close";
VAL_ 1041 PCS_INDICATOR 2 "PCS Faulted" 1 "PCS Turned Off By User" 0 "PCS Enabled";
VAL_ 1041 PCS_SENSITIVITY 64 "high sensitivity"  128 "mid sensitivity" 192 "low sensitivity" 0 "off";
VAL_ 1042 LDA_ALERT 3 "hold with continuous beep" 2 "LDA unavailable" 1 "hold" 0 "none";
VAL_ 1042 BARRIERS 3 "left" 2 "right" 1 "both" 0 "none";
VAL_ 1042 RIGHT_LINE 3 "orange" 2 "faded" 1 "solid" 0 "none";
VAL_ 1042 LKAS_STATUS 1 "on" 0 "off";
VAL_ 1042 LEFT_LINE 3 "orange" 2 "faded" 1 "solid" 0 "none";
VAL_ 1042 LDA_ON_MESSAGE 2 "Lane Departure Alert Turned ON, Steering Assist Inactive" 1 "Lane Departure Alert Turned ON, Steering Assist Active" 0 "clear";
VAL_ 1042 LDA_SA_TOGGLE  2 "steering assist off" 1 "steering assist on";
VAL_ 1042 LDA_SENSITIVITY 2 "standard" 1 "high" 0 "undefined";
VAL_ 1042 LDA_MESSAGES 4 "lda unavailable at this speed" 1 "lda unavailable below approx 50km/h" 0 "ok";
VAL_ 1042 LDA_FRONT_CAMERA_BLOCKED 1 "lda unavailable" 0 "ok";
VAL_ 1042 TAKE_CONTROL 1 "take control" 0 "ok";
VAL_ 1042 LANE_SWAY_WARNING 3 "ok" 2 "orange please take a break" 1 "prompt would you like to take a break" 0 "ok";
VAL_ 1042 LANE_SWAY_BUZZER 3 "ok" 2 "beep twice" 1 "beep twice" 0 "ok";
VAL_ 1161 TSGN1 1 "speed sign" 0 "none";
VAL_ 1161 TSGN2 1 "speed sign" 0 "none";
VAL_ 1161 SPLSGN2 15 "conditional blank" 4 "wet road" 5 "rain" 0 "none";
VAL_ 1162 TSGN3 0 "none" 1 "speed sign" 2 "0 unlimited" 7 "unlimited" 16 "highway" 17 "no highway" 18 "motorway" 19 "no motorway" 20 "in city" 21 "outside city" 22 "pedestrian area" 23 "no pedestrian area" 65 "no overtaking left" 66 "no overtaking right" 67 "overtaking allowed again" 81 "no right turn" 97 "stop" 105 "yield" 113 "stop" 114 "yield us" 129 "no entry" 138 "no entry tss2" 145 "do not enter";
VAL_ 1162 SPLSGN3 15 "conditional blank" 4 "wet road" 5 "rain" 0 "none";
VAL_ 1552 METER_SLIDER_LOW_BRIGHTNESS 1 "Low brightness mode, footwell lights off" 0 "Normal mode, footwell lights on";
VAL_ 1552 METER_SLIDER_DIMMED 1 "Dimmed" 0 "Not Dimmed";
VAL_ 1552 UNITS 1 "km (km/L)" 2 "km (L/100km)" 3 "miles (MPG US)" 4 "miles (MPG Imperial)";
VAL_ 1553 UNITS 1 "km" 2 "miles";
VAL_ 1556 TURN_SIGNALS 3 "none" 2 "right" 1 "left";
VAL_ 1556 BLINKER_BUTTON_PRESSED 1 "button pressed" 0 "not pressed";
VAL_ 1570 HEADLIGHT_MODE 0 "headlights off" 2 "force parking lights" 4 "force low beams" 7 "auto low beams" 6 "auto parking lights";
VAL_ 1592 LOCK_STATUS 0 "locked" 1 "unlocked";
