---
title: Smart Cruise Control - Vision
---

# Smart Cruise Control — Vision (SCC-V)

## What It Does

SCC-V uses the device's camera to detect lead vehicles and make smarter cruise control decisions. It provides vision-based adaptive speed adjustments for vehicles that rely on ICBM for cruise management.

## How It Works

The camera continuously monitors the road ahead. When a lead vehicle is detected, SCC-V adjusts cruise speed commands through [ICBM](icbm.md) to maintain safe following distances and react to speed changes of the vehicle ahead.

## Requirements

!!! info "Requirements"
    - [ICBM](icbm.md) must be enabled
    - Vehicle must support ICBM
    - Camera must have a clear view of the road ahead

## How to Enable

**Settings** → **Cruise** → **Smart Cruise Control — Vision**

## Settings Reference

See [Cruise Control Settings](../../settings/cruise/index.md) for configuration details.
