VERSION "ParkAssistCAN"


NS_ :
	NS_DESC_
	CM_
	BA_DEF_
	BA_
	VAL_
	CAT_DEF_
	CAT_
	FILTER
	BA_DEF_DEF_
	EV_DATA_
	ENVVAR_DATA_
	SGTYPE_
	SGTYPE_VAL_
	BA_DEF_SGTYPE_
	BA_SGTYPE_
	SIG_TYPE_REF_
	VAL_TABLE_
	SIG_GROUP_
	SIG_VALTYPE_
	SIGTYPE_VALTYPE_
	BO_TX_BU_
	BA_DEF_REL_
	BA_REL_
	BA_DEF_DEF_REL_
	BU_SG_REL_
	BU_EV_REL_
	BU_BO_REL_
	SG_MUL_VAL_

BS_:

BU_: ACM CGM EPAS_P ESP IBM OCS RCM SAS TestTool VDM Vector_XXX

BO_ 794 WheelButtons: 7 XXX
 SG_ LeftButton_ScrollClick : 19|2@0+ (1,0) [0|3] "" XXX
 SG_ LeftButton_RightClick : 21|2@0+ (1,0) [0|3] "" XXX
 SG_ LeftButton_LeftClick : 22|2@1+ (1,0) [0|3] "" XXX
 SG_ LeftButton_Scroll : 31|8@0+ (1,0) [0|255] "" XXX
 SG_ RightButton_ScrollClick : 35|2@0+ (1,0) [0|3] "" XXX
 SG_ RightButton_RightClick : 37|2@0+ (1,0) [0|3] "" XXX
 SG_ RightButton_LeftClick : 38|2@1+ (1,0) [0|3] "" XXX
 SG_ RightButton_Scroll : 47|8@0+ (1,0) [0|255] "" XXX

BO_ 848 BSM_BlindSpotIndicator: 4 XXX
 SG_ BSM_BlindSpotIndicator_Checksum : 0|8@1+ (1,0) [0|255] "" XXX
 SG_ BSM_BlindSpotIndicator_Counter : 11|4@0+ (1,0) [0|15] "" XXX
 SG_ BSM_BlindSpotIndicator_Left : 29|2@0+ (1,0) [0|3] "" XXX
 SG_ BSM_BlindSpotIndicator_Right : 30|2@1+ (1,0) [0|3] "" XXX

BO_ 4890 WheelButtons_Fwd: 7 XXX
 SG_ LeftButton_ScrollClick : 19|2@0+ (1,0) [0|3] "" XXX
 SG_ LeftButton_RightClick : 21|2@0+ (1,0) [0|3] "" XXX
 SG_ LeftButton_LeftClick : 22|2@1+ (1,0) [0|3] "" XXX
 SG_ LeftButton_Scroll : 31|8@0+ (1,0) [0|255] "" XXX
 SG_ RightButton_ScrollClick : 35|2@0+ (1,0) [0|3] "" XXX
 SG_ RightButton_RightClick : 37|2@0+ (1,0) [0|3] "" XXX
 SG_ RightButton_LeftClick : 38|2@1+ (1,0) [0|3] "" XXX
 SG_ RightButton_Scroll : 47|8@0+ (1,0) [0|255] "" XXX

BO_ 4944 BSM_BlindSpotIndicator_Fwd: 4 XXX
 SG_ BSM_BlindSpotIndicator_Checksum : 0|8@1+ (1,0) [0|255] "" XXX
 SG_ BSM_BlindSpotIndicator_Counter : 11|4@0+ (1,0) [0|15] "" XXX
 SG_ BSM_BlindSpotIndicator_Left : 29|2@0+ (1,0) [0|3] "" XXX
 SG_ BSM_BlindSpotIndicator_Right : 30|2@1+ (1,0) [0|3] "" XXX

VAL_ 848 BSM_BlindSpotIndicator_Left 0 "OFF" 1 "OBJECT_DETECTED" 2 "ACTIVE_WARNING" ;
VAL_ 848 BSM_BlindSpotIndicator_Right 0 "OFF" 1 "OBJECT_DETECTED" 2 "ACTIVE_WARNING" ;
VAL_ 4944 BSM_BlindSpotIndicator_Left 0 "OFF" 1 "OBJECT_DETECTED" 2 "ACTIVE_WARNING" ;
VAL_ 4944 BSM_BlindSpotIndicator_Right 0 "OFF" 1 "OBJECT_DETECTED" 2 "ACTIVE_WARNING" ;