---
title: Display Settings
---

# Display Settings

Control screen brightness, timing, and UI behavior for the onroad display.

**Location**: `Settings -> Display`

!!! info "Toggle & Device Availability"
    Supported on all devices. comma four users must use sunnylink to change this setting.

---

## Onroad Brightness

A selector that controls the screen brightness while driving. Use the **-** and **+** buttons to cycle through the options:

| Option | What it does |
|--------|-------------|
| **Auto (Default)** | Adjusts brightness automatically based on ambient light |
| **Auto (Dark)** | Adjusts automatically but biased toward a darker screen |
| **Screen Off** | Turns the screen off completely after the delay period |
| **0% - 100%** | Fixed brightness level in 5% increments |

---

## Onroad Brightness Delay

A selector that sets how long the screen stays at full brightness before the selected brightness mode takes effect. Available delay values range from seconds to minutes.

!!! note "Availability"
    This selector is disabled when Onroad Brightness is set to Auto (Default) or Auto (Dark), since those modes manage brightness continuously.

---

## Interactivity Timeout

A selector that controls how long the settings interface stays open before automatically closing and returning to the driving screen. Use the **-** and **+** buttons to choose a timeout:

| Option | Timeout |
|--------|---------|
| **Default** | Standard system timeout |
| **10s - 120s** | Custom timeout in 10-second increments |
| **1m / 2m** | One or two minute timeout |

---

## Related Features

- [Onroad Display](../features/display/onroad-display.md)
